|  |  |
| --- | --- |
|  | **Copper Electrolyzer** |
| Article number | BE05752 |
| EAN | 8714404039017 |
| Maximum pressure | 1 bar |
| Maximum flow | 13 m³/h |
| Diameter unit Ø | 59 mm |
| Copper Ionizer | 0,7 ppm |
| Length unit | 34 cm |
| In/outlet connections Ø | 48/50 mm |
| Housing material | PC/ASA |
| Electronic ballast | 230 V AC 50 Hz |

Technical specifications

*Pending EU regulations or conditional approval, national regulations apply to the trade and use of copper-containing products. The copper used in these units complies with the REACH registration. It is the sole responsibility of the buyer to inform himself/herself about applicable local regulations regarding the use of (and trade in) copper for water disinfection.*