|  |  |
| --- | --- |
|  | **120 V (Type B)** |
| Article number | 5056584 |
| Type | Type B |
| EAN | 8714404044622 |
| Voltage | 120 V AC |
| Frequency | 60 Hz |
| IP Class | 54 |
| Connection size, tee fitting | 2" |
| Minimum flow | 1,5 m3/h |
| Maximum flow | 23 m3/h |

Technical specifications