Technical specifications

|  |  |  |
| --- | --- | --- |
|  | **40 W** | **75 W** |
| Article number | BH04402 | BH04752 |
| Type | 40 W | 75 W |
| EAN | 8714404034241 | 8714404036689 |
| Maximum flow for 30 mJ/cm2 | 11 m3/h | 16 m3/h |
| Maximum pressure | 2 bar | 2 bar |
| Diameter unit Ø | 70 mm | 70 mm |
| Length unit | 100 cm | 100 cm |
| In/outlet connections Ø | 63 mm/50 mm/1½” BSPP female | 63 mm/50 mm/1½” BSPP female |
| Housing material | AISI 316L | AISI 316L |
| Lifespan lamp | 9 000 hours | 9 000 hours |
| Copper ionizer | 0,7 ppm | 0,7 ppm |
| Replace lamp alert | √ | √ |
|  |  |  |

*Pending EU regulations or conditional approval, national regulations apply to the trade and use of copper-containing products. The copper used in these units complies with the REACH registration. It is the sole responsibility of the buyer to inform himself/herself about applicable local regulations regarding the use of (and trade in) copper for water disinfection.*