# Inox UV-C

Advantages

* Complete 316L Stainless steel housing
* Standard equipped with flow switch for safe operation
* Integrated timer indicates when lamp replacement is needed
* Handles up to 5 bar pressure for robust performance
* Efficient UV-C treatment in 316L Stainless steel housing