Technical specifications

|  |  |  |
| --- | --- | --- |
|  | **75 W** | **130 W Amalgam** |
| Article number | BP02752 | BP02132 |
| Type | 75 W | 130 W Amalgam |
| EAN | 8714404038669 | 8714404038676 |
| Maximum flow for 30 mJ/cm2 | 18 m3/h | 22 m3/h |
| Maximum pressure | 5 bar | 5 bar |
| Diameter unit Ø | 114 mm | 114 mm |
| Length unit | 100 cm | 100 cm |
| In/outlet connections Ø | 2” BSPT male | 2” BSPT male |
| Housing material | AISI 316L | AISI 316L |
| Lifespan lamp | 9 000 hours | 12.000 hours |
| Timer | √ | √ |
| Replace lamp alert | √ | √ |
| Flow switch | √ | √ |