Technical specifications

|  |  |  |  |
| --- | --- | --- | --- |
|  | **40 W** | **75 W** | **130 W Amalgam** |
| Article number | BD01402 | BD01752 | BD01132 |
| Type | 40 W | 75 W | 130 W Amalgam |
| EAN | 8714404040501 | 8714404040570 | 8714404040648 |
| Maximum flow for 30 mJ/cm2 | 11 m3/h | 16 m3/h | 22 m3/h |
| Maximum pressure | 2 bar | 2 bar | 2 bar |
| Diameter unit Ø | 70 mm | 70 mm | 70 mm |
| Length unit | 100 cm | 100 cm | 100 cm |
| In/outlet connections Ø | 63 mm/50 mm/1½” BSPP female | 63 mm/50 mm/1½” BSPP female | 63 mm/50 mm/1½” BSPP female |
| Housing material | Duplex | Duplex | Duplex |
| Lifespan lamp | 9 000 hours | 9 000 hours | 16 000 hours |
| Timer | √ | √ | √ |
| Replace lamp alert | √ | √ | √ |
| Flow switch | No | No | √ |