Spare parts

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  | Available for: | **80 W**  **Ø 114** | **140 W  Ø 114** | **140 W Ø 154** | **420 W**  **Ø 219** |
| A | F980010 | F980010AM Lamp VGE T5 80 W 4P Base X AM Packed | √ |  |  |  |
| F980020 | F980020AM Lamp VGE T6 140 W 4P Base X AM Packed |  | √ | √ | √ |
| B | QG075 | Quartz glass VSC 870 x 30 mm AM | √ | √ | √ | √ |
| C | E800912 | Set O-ring for quartz glass | √ | √ | √ | √ |
| D | EP080020 | Electrics Xpert Buster UV-C 80 W | √ |  |  |  |
| EP130016 | Electrics Xpert Buster UV-C 140 W  incl. flow switch |  | √ | √ |  |
| EP390005 | Electrics Xpert Buster UV-C 420 W  incl. flow switch |  |  |  | √ |
| E | B212130 | Housing Xpert Buster UV-C Ø 114 mm | √ | √ |  |  |
| B212131 | Housing Xpert Buster UV-C Ø 154 mm |  |  | √ |  |
| B212120 | Housing Xpert Buster UV-C Ø 219 mm |  |  |  | √ |
| M | B290020 | Reduction piece 63/63 mm 3/4” male threaded for flow switch |  | √ | √ | √ |
| B290021 | Reduction piece 60.3/60.3 mm 3/4”  USA-UK male threaded for flow switch |  | √ | √ | √ |
| U | E801533 | Adjustable foot stainless steel M8 | √ | √ | √ | √ |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  | Optional |  |  |  |  |  |
| V | B290177 | Tapping saddle 50 x 3/4" male thread for flow switch | | |  |  |
| B290170 | Tapping saddle 63 x 3/4" male thread for flow switch | | |  |  |
| B290176 | Tapping saddle 75 x 3/4" male thread for flow switch | | |  |  |