Technical specifications

|  |  |  |
| --- | --- | --- |
|  | **80 W** | **140 W Amalgam** |
| Article number | BP08752 | BP08132 |
| Type | 80 W | 140 W Amalgam |
| EAN | 8714404046329 | 8714404980920 |
| Maximum flow for 30 mJ/cm2 | 17 m3/h | 23 m3/h |
| Maximum pressure | 2,5 bar | 2,5 bar |
| Diameter unit Ø | 70 mm | 70 mm |
| Length unit | 100 cm | 100 cm |
| In/outlet connections Ø | 63 mm/50 mm/1½” BSPP female | 63 mm/50 mm/1½” BSPP female |
| Housing material | Duplex | Duplex |
| Lifespan lamp | 9 000 hours | 16 000 hours |
| Indicator | √ | √ |
| Replace lamp alert | √ | √ |
| Flow switch | No | √ |