Technial specifications

|  |  |
| --- | --- |
|  | **1500 W** |
| Article number | BPM01501 |
| Type | 1500-168 |
| EAN | 871440404726 |
| Maximum rated pressure | 10 bar |
| Flow 400 J/m2 (Disinfection) | 107 m³/h |
| Flow 600 J/m2 (Chloramine reduction) | 62 m³/h |
| In/outlet connections Ø | DN150 flange |
| Housing material | AISI 316L |
| Control panel | Compact |
| Lifespan lamp | 9 000 hours |
| Temperature switch | √ |
| Lamp function indicator | √ |
| Replace lamp alert | √ |
| Flow switch | Optionally connectable but not included |