Technical specifications

|  |  |
| --- | --- |
|  | **230 V (Type F)** |
| Article number | 5056579 |
| Type | Type F |
| EAN | 8714404044486 |
| Voltage | 230 V AC |
| Frequency | 50 Hz |
| IP Class | 54 |
| Connection size, tee fitting | 63 mm |
| Minimum flow | 1,5 m3/h |
| Maximum flow | 23 m3/h |