Technical specifications

|  |  |
| --- | --- |
|  | **230 V (Type G)** |
| Article number | 5056587 |
| Type | Type G |
| EAN | 8714404044936 |
| Voltage | 230 V AC |
| Frequency | 50 Hz |
| wwIP Class | 54 |
| Connection size, tee fitting | 63 mm |
| Minimum flow | 1,5 m3/h |
| Maximum flow | 23 m3/h |