# Copper Ionizer UV-C

Advantages

* Combines copper ionization with UV-C for enhanced disinfection
* Copper ions help prevent algae growth and reduce chemical use
* 316L Stainless steel housing for maximum corrosion resistance
* Easy to install and maintain, minimizing downtime
* Universal fittings included (63mm/50mm/1½” BSPP female)