# Tech UV-C 4ALL

Advantages

* Suitable for all pools
* Durable duplex Stainless steel
* Corrosion & chlorine resistant
* Horizontal or vertical installation possible
* Fits in new & existing pool filtration systems
* Universal fittings included (63 mm/50 mm/1½”)
* Optimized flow with minimal pressure loss