# Tech UV-C

Advantages

* Easy to install and maintain, minimizing downtime
* 316L Stainless steel housing
* Universal fittings included (63mm/50mm/1½” BSPP female)
* Efficient UV-C treatment ensures clean and healthy water