# Timer UV-C 4ALL

Advantages

* Timer function indicates when lamp needs replacement
* Suitable for all pools
* Durable duplex Stainless steel
* Corrosion resistant
* Horizontal or vertical installation possible
* Fits in new & existing pool filtration systems
* Universal fittings included (63mm/50mm/1½” BSPP female)
* Optimized flow with minimal pressure loss