# SPAOP UV

Advantages

* Cost-efficient: UV initiated radical generation eliminates the need for Ozone
* Combines oxidation and disinfection with OH-radicals and UV for superior water quality
* High-energy UV at 185 nm enhances color, smell and clarity
* Compact and easy to integrate into existing spa systems
* Maximum disinfection effectiveness with minimal chemical use
* Stand-alone unit with LED indicator for easy monitoring
* Designed for safe operation up to 40°C/104°F