# Buster UV-C

Advantages

* Can be mounted horizontally or vertically for flexible installation
* Large chamber ensures long UV contact time for clean and healthy water
* 316L Stainless steel chamber for corrosion and chlorine resistance
* Transparent lamp head allows easy visual check of system operation
* Handles higher water flows for efficient treatment of larger pool volumes