# Duplex UV-C

Advantages

* Suitable for all pools
* 140 Watt Amalgam unit includes flow switch for safe operation
* Multiple installation options for easy installation and integration
* Efficient UV-C treatment for healthy and clear water
* Universal fittings included (63mm/50mm/1½” BSPP female)
* Stand-alone electrical part